HUAQIN BMC Readme

## **Release Summary**

**Platform:** Mehlow

**Project Name:** SR2515

The contents of this package contains the following components

.\ A30803B0012\_Readme.docx – This file Providing applications and usage notes for released update.

.\Linux – Provides SOC Flash tool under Linux

.\Shell – Provides SOC Flash tool under UEFI Shell

.\Windows – Provides SOC Flash tool under Windows

.\File – This folder provides release notes, IMA firmware, and firmware MD5 checksum

.\ FWUPDATE\_BMC\_DOS.BAT – Provides update scripts that can be executed directly under DOS

.\ fwupdate\_bmc\_linux.sh – Provides update scripts that can be executed directly under Linux

.\ fwupdate\_bmc\_shell.nsh – Provides update scripts that can be executed directly under UEFI Shell

.\ fwupdate\_bmc\_win.bat – Provides update scripts that can be executed directly under Windows

## Update Instructions

Firmware:

When need flash BMC on windows, please run fwupdate\_bmc\_win.bat.

When need flash BMC on Dos, please run FWUPDATE\_BMC\_DOS.BAT

When need flash BMC on Linux, please run fwupdate\_bmc\_linux.sh

When need flash BMC on UEFI Shell, please run fwupdate\_bmc\_shell.nsh

Notes:

When using fwupdate.bat flash BMC on DOS, Need change BIOS uefi mode to legacy mode.

# Steps after BMC Update

The steps given is only needed for the BMC upgrade from BMC version lower than A30803B0001 to higher.

1) After flashing the latest BMC using WEB.

2) Login using the user "ADMIN/ADMIN".

3) Do a factory reset in Web.

4) Wait for the Reset